Determination of Pointing Parameters IRAM Plateau de Bure Interferometer

S. Guilloteau^1 February 4, 2002

Version 2.0 (1) Institut de Radio Astronomie Millimétrique 300 Rue de la Piscine F-38406 Saint Martin d’Hères This document describes the current tools for determining the pointing of the antennas on Plateau de Bure. Good pointing is essential to the operation of the interferometer. Unfortunately, there are many ways to do bad or poor pointing, and no simple way to do it well. Please read this document carefully . Its contents are important.

This document is a sum up of the steps relevant for pointing. More details on the individual programs and command mentionned in this document are available in:

ffl IRAM Plateau de Bure Interferometer: Introduction ffl IRAM Plateau de Bure Interferometer: OBS Users Guide ffl CLASS Users Guide ffl CLIC Users Guide ffl SIC and GreG Users Guide

2 CONTENTS

Contents

1 Basic pointing parameters 3 1.1 Parameter List . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3 1.2 Parameter Files . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4

2 The POINT program 4 2.1 Description . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4 2.2 Optical versus Radio . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6

3 Optical Pointing 6 3.1 Getting data . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6 3.2 Optical Pointing using MNU . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6 3.3 Reducing data . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7

4 Radio Pointing 8 4.1 Full sky, single-dish radio pointing . . . . . . . . . . . . . . . . . . . . . . . . . 8 4.2 Interferometer pointing . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 8 4.3 Limited radio pointing determination . . . . . . . . . . . . . . . . . . . . . . . 9

5 Inclinometers 9

6 Cookbook, Tricks, and Traps 9

7 POINTn Language Help 11 7.1 FILE . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11 7.2 IGNORE . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11 7.3 INCLUDE . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11 7.4 LIST . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11 7.5 PARAMETER . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11 7.6 PLOT . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 12 7.7 PRINT . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 13 7.8 READ . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 13 7.9 REJECT . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 13 7.10 SET . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 13 7.11 SHOW . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 14 7.12 SOLVE . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 14

1 Basic pointing parameters

1.1 Parameter List

Let dX and dY be the offsets on the sky parallel to the Azimuth axis and Elevation axis respectively, produced by a pointing error. The standard pointing model for the Plateau de Bure antennas has the following parameters:

IAZ azimuth encoder zero
         dX = IAZ*cos(El) dY = 0
IEL elevation encoder zero
         dX = 0 dY = IEL
COH telescope azimuth collimation
         dX = cos(El)*asin(COH/cos(El)) dY = -asin(sin(El)/sqrt(1-COH**2))
         for COH << cos(El), equivalent to
         dX = COH dY = 0,
COV telescope vertical collimation
         dX = 0 dY = COV
MVE Azimuth axis tilt towards East
         dX = MVE*cos(Az)*sin(El) dY = -MVE*sin(Az)
MVN Azimuth axis tilt towards North
         dX = -MVN*sin(Az)*sin(El) dY = -MVN*cos(Az)
NPE Elevation axis tilt (axis non perpendicularity)
         dX = -NPE*sin(El) dY = 0
         (assuming small NPE and COH in practice.)
REF0 First order refraction coefficient
         dX = 0 dY = -REF0/tan(El)
REF1 Second order refraction coefficient
         dX = 0 dY = -REF1/tan(El)**3
ELES gravity+eccentricity of Elevation encoder
         dX = 0 dY = ELES*sin(El)
ELEC gravity+eccentricity of Elevation encoder
         dX = 0 dY = ELEC*cos(El)
AZES eccentricity of Azimuth encoder
         dX = AZES*sin(Az)*cos(El) dY = 0
AZEC eccentricity of Azimuth encoder
         dX = AZEC*cos(Az)*cos(El) dY = 0
HEL Homology elevation bending (cos(El))
         dX = 0 dY = -HEL*cos(El)

The total pointing correction is thus, in the small COH approximation

dX = IAZ.cos(El) + COH + sin(El) * (MVE*cos(Az)-MVN*sin(Az)-NPE)
      + cos(El) * (AZES*sin(Az)+AZEC*cos(Az))
dY = IEL+COV - (MVE*sin(Az)+MVN*cos(Az))
      + (ELES*sin(El)+(ELEC-HEL)*cos(El))
      - REF0/tan(El) - REF1/tan(El)**3 - REF2/tan(El)**5

Since each antenna is equipped with an off-axis optical telescope, there are two sets of

(COH,COV) values, one for the radio axis and one for the optical axis. As only IEL+COV is

meaningful, the radio COV is set to zero, fixing the IEL value.

4 2 THE POINT PROGRAM

Five terms dominate the pointing model : IAZ, IEL+COV, COH, MVE and MVN. In principle

COH, IEL, and COV depend only on the antenna, MVE and MVN depend on the station and antenna

(azimuth bearing), and IAZ depends on the antenna (encoder), the station (footpad positions) and the positioning of the antenna on the station (repeatability 1 mm).

The refraction coefficients are weather dependant. Accordingly, the parameters are computed in real time, using temperature, pressure and humidity. REF0 and REF1 are thus fixed to zero in the pointing fit.

Among the other terms, all of which depend on the antenna, just two have been found to be of some importance for some antennas: ELEC which enters only in combination with HEL in radio (small values on all antennas), and possibly NPE (Antenna 3). These are marginally different from zero, however, and confirmation will be required. The other parameters can be set to zero.

1.2 Parameter Files

The values for these parameters used in real time are stored in several parameter files, located under directory INTER BASE:. To follow the logical dependence of the parameters upon antenna and station, several files exist :

ffl GENERAL.ANk

where k is an antenna number. These files contain the parameters which only depends on the antenna: radio and optical collimations COH and COV, NPE, AZEC, AZES, ELEC, ELES, and also a default value for IAZ. They also contain the homology elevation bending, HEL, the subreflector parameters: HTR0 and HTR1 for translation, HVT0 and HVT1 for tilt, HFO0 and HFO1 for focus; and two beam-switch parameters (sign and beam separation).

ffl Sij.ANk

where Sij is a station name (for example W00), and k an antenna number. These files contains the Antenna-Station dependent parameters, for pointing IAZ, MVE, and MVN, and for interferometry, the Delay, and the position X,Y,Z.

The Sij.ANk should never be editted, but should only be changed using the CONFIGURE mode of OBS. The GENERAL.ANk file should be editted if a major change occur.

2 The POINT program

2.1 Description

The POINT program is a pointing parameter fitting program based on the SIC user interface, and GreG for graphic display. It is called by the command:

$ POINT

A typical session with POINT is:

ffl GREG1nDEVICE RETRO

Define graphic device for display

ffl FILE 16-OCT-1989 RADIO

Define the input data file and type. Three data types exist: RADIO, for single-dish radio pointing results, INTER for interferometric pointing results, and OPTICAL for optical

2.1 Description 5

pointing data. The file extension is derived from the data type using the following defaults : .RAD, .INT and .OPT respectively. .RAD files are produced by the CLASS

ANALYSEnPRINT POINTING command, .INT files are produced by the CLIC CLICnSOLVE
POINTING command, and .OPT files are produced by the DCL SAV command on the real-

time microVAX BURE01. The data type also defines the default variable parameters.

ffl READ 2

Read the data for Antenna 2 from the input file.

ffl SOLVE

Solve for the pointing parameters using the currently read data.

ffl PLOT SUMMARY

Display on the graphic device a summary of residual pointing errors; residual in Elevation versus residual in Azimuth.

ffl PLOT COVERAGE

Display the Azimuth and Elevation coverage to see whether correlated parameters, such as

IAZ and COH for example, are well determined or not.

ffl PRINT/OUTPUT 16-OCT-1989.RADIO/HEADER

If both the summary and coverage look good, write the fit results to a file for the archive. The /HEADER option is used to write out the values of the fixed parameter also.

If some points appear discrepant in the fit or if the fit residuals are large, there are several possibilities for rejecting bad data points.

ffl REJECT 8.0

Reject all data points with pointing residuals higher than 8:0” after the last SOLVE command.

ffl SET RMS 2.0

Select only those data points for which the formal error on the pointing observation is less than 2:0”. For INTER and RADIO data types, the formal error is computed by the CLIC and CLASS gauss fit commands, and the error is set to zero for OPTICAL data.

ffl SET ELEVATION 10.0 80.0

Select only data points in the elevation range 10 to 80 degrees. The default elevation range is 5 to 90 degrees.

ffl IGNORE/SCAN s1 s2 s3 TO s4 BY s5/SOURCE JUPITER

Ignore some scans in the data (the scan numbers are displayed by the PLOT SUMMARY command), or some sources. Previously ignored scans and sources can be reconsidered agin using the INCLUDE command (same syntax as IGNORE).

If the coverage is bad, it is interesting to fix some parameter to reduce the errors on correlated parameters. This is especially true for the radio COH, because the collimation is essentially a constant that depends only on the antenna. For example

ffl PARAMETER COH 42.0

Will fix COH to 42”.

ffl PARAMETER MVE/FREE

Will free the (previously fixed) parameter MVE.

6 3 OPTICAL POINTING

2.2 Optical versus Radio

The types of data files treated by POINT differ slightly. For Optical data, the pointing error is relative to a perfect antenna. Hence the POINTnPRINT output directly indicates the new pointing parameter values. For Radio (or Interferometer) data, however, the pointing error is relative to the previous model, except for the collimations. Hence POINTnPRINT yields directly COH and COV, but for all other parameters the POINT results should be added to the previous values.

In particular, the Radio results can be used in the OBS SETnPOINTING command in an incremental way:

SET\POINTING IAZ IAZ+dIaz IEL IEL+dIel/ANTENNA 2

where dIaz, dIel are the results given by command POINTnPRINT for the parameters IAZ, IEL.

3 Optical Pointing

3.1 Getting data

Optical pointing is done using the MNU program, and the DCL commands CRE (CREate the data file), SAV (SAVe telescope coordinates in the data file), CAT (select a star from the star CATalog), and PLA (select a PLAnet), or using the automatic searching mode of MNU. Please refer to the document “Foreign Commands” by A. Perrigouard for a complete description of these commands.

Two different approaches can be used for the optical pointing, depending whether you have an idea of the pointing parameters or not.

ffl First, make a crude optical pointing with a few stars, 5-8 at low and 3-6 at high elevations, with good azimuth coverage. The accuracy need not be very good (5”). Then, use the newly determined pointing constants to make a more accurate pointing session with 40 to 60 stars. All stars should be rather well centered already , and now the centering accuracy can be made better (1”). Uniform coverage is not required: most important is to have low and high elevation sources.

ffl Or use only a single pass with 60 stars centered within 1”. This can take somewhat longer because the stars may be far off center.

3.2 Optical Pointing using MNU

MNU includes a mode for optical pointing, accessible through the REFLECTOR page:

GOLD HELP POINT REMOTE
/DEF /TOP /STOP MICRO
C.SYS Tracking
/HORI SPI. GUID. OFFS.
       Second. Mirror
FOCUS TRANS V TILT H TILT
SAVE NEXT
        /DIST SLEW MNU
INIT ANT. REF. RAD ANTEN.
/SUB REF. /OPTIC

3.3 Reducing data 7

In this mode, activated by the POINT key (PF3 on the REFLECTOR page), it tries to find the best candidates to map the sky uniformly in azimuth and elevation. The density of stars is given by specifying the minimal distance angle between stars, using the GOLD/DISTANCE (PF1/KP2) key. To hasten a pointing session, the program will try to find candidates above 10 degrees in elevation and at the minimum distance (in time) from the current telescope position.

MNU uses a catalog of bright stars named J2000R.CAT in the [CONTROL.COMMAND] directory, on disk COMP$DISK:, and writes the pointing data in the most recently created Date.OPT file on directory [OBSERVER.POINTING], on disk RLTDATA (Date being a date in format DD-MMM-YYYY as usual). The file POINTING.OPT, also in [OB- SERVER.POINTING], contains the name of the last pointing data file created along with its creation time. MNU assumes that the pointing concerns the default antenna. To find out or modify this default use the DCL command DEF [Ant], or use the GOLD/DEF (PF1/PF1) key to change it.

To start an optical pointing session, press the POINT key. The program opens the data file Date.OPT, reads and processes the records concerning the default antenna, and then closes the file. It opens the catalog file J2000R.CAT and processes the star coordinates in order to prepare and to speed up the calculations next to be performed. Next, the file is closed.

Specify a minimum distance between stars using the GOLD/DISTANCE key, for instance 10.0 for 10 degrees. MNU will look for the best candidate, given the present telescope position, the data already saved in Date.OPT, and the possible stars in the catalog file. To move to the next star, press the NEXT (KP2) key.

When the telescope stops slewing and tracks the star, use MNU to move the telescope slightly so the TV cross-hair is on the star. Meanwhile, as soon as the command to send the telescope to the requested position has been spawned, the catalog is searched for the next star candidate. Once the TV cross-hair is on the star, press the SAVE (KP1) key to append the star position, the current telescope position, the sidereal time and the refraction correction to the data file. If an error occurs while opening the file, the operation can be executed again.

Then go on using the NEXT key... Every time you press the NEXT key, a message saying “No more candidate” may appear. You should then either suspend your pointing sessions using the GOLD/STOP (PF1/PF3) key, or decrease the minimal distance between stars using the

GOLD/DISTANCE (PF1/KP2) key.

3.3 Reducing data

To reduce optical pointing data, work on BURE02, in the [OBS.POINTING] directory, and use POINT, specifying the RLTDATA:[OBSERVER.POINTING]Date.OPT file as input:

$ SET DEF [OBS.POINTING]
$ POINT
POINT> FILE Date OPTICAL
POINT> READ Antenna_Number
POINT> SOLVE
POINT> [ Other commands ]

The file is fetch by default from directory RLTDATA:[OBSERVER.POINTING]. A fit will be made with the free parameters IAZ IEL+COV COH MVE MVN, and all other parameters fixed at zero. A fit with more free parameters (e.g. ELEC and NPE) can be made using the commands :

POINT> PARAMETER NPE/FREE
POINT> PARAMETER ELEC/FREE

8 4 RADIO POINTING

Optical pointing gives only the sum IEL+COV. The zero of the elevation encoder is an antenna constant. After a fit by POINT all parameters should be replaced in the antenna-station parameter file.

4 Radio Pointing

4.1 Full sky, single-dish radio pointing

If the radio pointing has to be determined for the first time (new antenna, new receiver, new subreflector alignment, or other major changes), a full sky radio pointing is necessary. Using the OBS OBSnPOINT command, observe 30 to 40 positions, preferably clustered at high and low elevations, but well spaced in azimuth.

Use CLASS on BURE02 to reduce the pointing measurements, working on the [OBS.SINGLE] directory. A procedure named PR:INIT POINT can be used in CLASS to get started. Open the .BUR input file, get a list of the pointing scan, using commands FIND and LIST. Then the procedure PR:POINT can be used to process the data scan by scan. For each pointing scan, it averages separately the two azimuth and two elevation subscans, fit gaussians, with two coupled components in case of beam switching, to the averages, and at each PAUSE, the user can write the result in an output data file, named Date.BUR-POINT. This can be done while data acquisition is still going on. Once all data have been reduced, open the reduced data file in input, select all data using the LASnFIND command, and then use ANALYSEnPRINT POINT/OUTPUT

[-.POINTING]Date.RAD to write out the fit results.

Stop CLASS and move to [OBS.POINTING] directory to use POINT to fit the pointing parameters. The default adjustable parameters are IAZ, IEL+COV, MVE, and MVN, while COH is set to its antenna dependent value, found from file INTER BASE:GENERAL.ANk.

In RADIO mode, POINT gives variations from the previous parameter values, except for COH where it gives the absolute value (note COV = dIEL, the variation of IEL). Refraction parameters should always be fixed to zero, since the radio refraction is computed in real time.

4.2 Interferometer pointing

Pointing sources can be observed with the OBS command

OBS\POINT /ANTENNA Iant /LENGTH 60

in INTERferometry mode if only antenna Iant is to be pointed, or

OBS\POINT /LENGTH 40

if all antennas must be pointed.

Data reduction can then be done with the CLICnSOLVE POINTING command in CLIC, working on the [OBS.POINTING] directory. Select a set of pointing scans with the CLICnFIND command (use SET PROCEDURE POINT) and process these scans with CLICnSOLVE POINTING [/PLOT]

/OUTPUT Date.INT. By default data is appended to that file, add argument NEW after the

Date.INT file name to create a new one.

For continuum sources, you should use SET SUB C01 TO C10 and SET AVERAGE METHOD

VECTOR. You might want to do an RF PASSBAND calibration to be able to average both side-

bands (SET RF ON, SET BAND AVERAGE); this is absolutely necessary at high frequencies to improve signal to noise ratio. If observing SiO masers at the standard frequency (86.051 USB LOW), use SET SUB C02 and SET BAND UPPER to process the data in CLIC.

Then, use POINT the same way as for the RADIO (single-dish) data.

4.3 Limited radio pointing determination 9

4.3 Limited radio pointing determination

Once the optical pointing parameters have been determined and entered in the Antenna-Station file, only one radio pointing on a strong source is needed to get the radio COV and the radio IAZ. The radio COH should be set to its (antenna-only dependent) value.

If the optical COV was already well known, you should find the radio COV = 0. Radio IAZ is determined as follows: measure the azimuth pointing error, divide it by cos(Elevation), and subtract the result from IAZ (Oui, soustraire). You should then be ready for a radio observing ! 5 Inclinometers

All antennas are equipped with one inclinometer, that should allow determination of the inclinations without astronomical pointing. Regular monitoring of the inclinometer outputs must be made. It is especially important to get the inclinometer results before and after each pointing session. To use the inclinometers:

ffl Send an antenna North at some elevation, chosen to avoid the sun at any azimuth, for example using antenna Iant

$ COO ANTE Iant HO 180D 85D NULL, under DCL, or
OBSnSOURCE INCLINO, OBSnLOAD, within OBS

ffl Once the antenna stops, run the inclinometer program

$ INC Iant /PLOT

The antenna will do a full turn at the current elevation, and a sine curve will be fit to the inclinations measured every 5 degrees. From this fit, the parameters MVE and MVN are derived from the azimuth axis tilt measured by the inclinometers using three additional corrections:

ffl a change of sign due to conventions on the orientation of the vertical.

ffl a local vertical correction to refer the inclinations to the vertical of the array center

ffl a global gravity corrections of MVE = +10”, MVN = +7”, to correct for large scale deviations of the gravity field due to the Alps.

The resulting MVE and MVN are displayed and written in the file INTER BASE:INCLINO.ANi, where i = Iant. The fit is displayed by GreG if you specified the /PLOT option for the INC command. A hardcopy possibility is offered.

6 Cookbook, Tricks, and Traps

It is difficult to produce a cookbook recipe for getting the pointing parameters. The following Traps should be avoided, however:

ffl Azimuth Elevation coverage

It MUST be reasonable. Never believe the formal errors on MVE or MVN if the Azimuth coverage is less than 270 degrees. Never believe the formal error on COH if the elevation coverage is less than 60 degrees. From the pointing error equations, it can be seen that the best coverage consists in sources equally spaced in Azimuth, but clustered at high and low elevations.

10 6 COOKBOOK, TRICKS, AND TRAPS

ffl Radio Collimation COH

This is essentially an antenna constant. It is better to fix COH to the previous value, rather than trying to fit it (see the INTER BASE:GENERAL.ANi file to get this number). Accordingly, this is done by default. Do not believe COH has changed unless you have 1) many data points

(¿ 40) 2) a good sky coverage, and 3) a formal error on COH less than 0:5”.

ffl Gauss fit formal error

For radio pointing, if the formal error on the position from gauss fit is higher than 2:0”, the data may be useless.

ffl Avoid long pointing sessions and systematic Az-El coverage At least in OPTICAL pointing. Time dependent effects, such as thermal behaviour of the optical telescope mount, may then become inextricably mixed with Az or El dependent terms.

Accordingly, the following Tricks should be used:

ffl Use SiO Masers in Pseudo Continuum

They will help you get a good Az-El coverage. They are usually stronger than continuum sources.

ffl Use the beam switch

Always for continuum sources, but also for SiO masers if the weather is poor.

ffl Fix the beam width for CLASS gauss fits

This helps to reduce the formal error on the position, specially for weak sources. This can be done using the CLASS command ANALYZEnMETHOD CONTINUUM Width, where Width is in arc seconds. The beam width is 55” at 86 GHz. The PR:INIT POINT.CLASS procedure executes such a command if the observing frequency is specified.

ffl Use the inclinometers

At least just before and just after the pointing session, but also later from time to time to check any time dependence of MVE or MVN.

ffl Use the specially designed procedure POINT INTER and POINT MULTI These procedures have been written to produce a reasonable coverage, considering the functional form of the pointing model equations. Pointing sources have been selected to avoid excessive noise.

7 POINTn Language Help

7.1 FILE

    [POINT\]FILE Name Type

     Specify the input file name and type of data (OPTICAL, RADIO or
INTERFEROMETRY). The file extension is derived according to Type using
the following defaults : .OPT, .RAD and .INT respectively. The file
header are read, but not the data.

7.2 IGNORE

    [POINT\]IGNORE [/SCAN List of scans] [/SOURCE List of sources]
[/TIME TimeMin TimeMax]

     Ignore part of the input data for the next SOLVE command. The data
must have been read before. The Scan list, Source list and time ranges
are emptied each time a new READ or FILE command is typed.

7.3 INCLUDE

     [POINT\]INCLUDE [/SCAN List of scans] [/SOURCE List of source]
[/TIME Tmin Tmax]

     Include part of the input data (presumably previously ignored) for
the next minimization. The data must have been read before. The Scan
list or Source list can be replaced by the "wildcard" * to include any
scan or source.

7.4 LIST

    [POINT\]LIST [Scan] [/OUTPUT Filename]

     List the current data or the specified scan. The bad data is
flagged with an exclamation point. Option /OUTPUT can be used to
redirect the LIST command output (default Terminal).

7.5 PARAMETER

    [POINT\]PARAMETER NAME [Value] [/FREE]

     Fix a fit parameter at the specified value, or free the specified
parameter if option /FREE is present. Value is in arcsecond. Available
parameters are
      IAZ Zero azimuth

      IEL+COV Zero elevation
      COH Azimuth collimation
      MVE East Inclination
      MVN North Inclination
      NPE Non perpendicularity
      REF1 1st order refraction
      REF2 2nd order refraction
      ELES grav.+exc. coder ele. (sin)
      ELEC grav.+exc. coder ele. (cos)
      AZES excen. coder az. (sin)
      AZEC excen. coder az. (cos)
REF1 and REF2 are preset to 0 and 0 by default, because on Plateau de
Bure the refraction is computed in real from meteo parameters. They
should not be freed, except for very specific purposes.

7.6 PLOT

              PLOT [Argument] [/BAD]

     Plot some aspect of the data and fit results. Argument may be
         SUMMARY (Default).
         Residuals in El versus residuals in Az.

         COVERAGE
         Elevation versus Azimuth of data points.

         ERRORS AZIMUTH or ERRORS ELEVATION
         Original pointing errors in Az or El, as a function of Az and
         El.

         RESIDUALS AZIMUTH or RESIDUALS ELEVATION
         Residual pointing errors in Az or El, as a function of Az and
         El.

         TIME
         Residual pointing errors as a function of time.

         CIRCLE
         General summary of pointing behaviour : arrows indicating the
         pointing error magnitude and direction on a (Az,El) circular
         diagram.
By default, only good data points (those considered for the fit) are
plotted. If option /BAD is present, rejected data points (as
implicitely specified by commands IGNORE, REJECT, SET ELEVATION and SET
RMS) are also plotted, using the virtual pen number 2.

7.7 PRINT 13

7.7 PRINT

    [POINT\]PRINT [/OUTPUT Filename|PRINTER] [/HEADER]

     List the last fit results computed by command SOLVE. Option
/HEADER can be used to list all fit parameters; by default only variable
parameters are listed. Option /OUTPUT can be used to redirect the PRINT
command output (default Terminal); if PRINTER is specified as argument
to /OUPUT option, the fit results are printed.

7.8 READ

    [POINT\]READ Antenna0mber [Station0me]

     Read the data of antenna Antenna0mber (on station Station0me if
specified). A file must have been opened using command FILE before.

7.9 REJECT

    [POINT\]REJECT MaxError

     Reject all data points with pointing residuals greater than
MaxError for the next fits. A READ command will reset the rejection
threshold to infinity.

7.10 SET

    [POINT\]SET Item Value1 [Value2]

     Set some selection criterium. Possible items are
         ELEVATION Elmin Elmax :
         specify valid elevation range (default 5 90, in degrees)

         RMS rmsmax :
         specify maximum standard deviation (from gauss fit) for the
         measured pointing errors.
Optical pointing data has measured pointing errors with standard
deviation set to 0, so that SET RMS although meaningfull only for RADIO
or INTER data, can also be used transparently.

     As for comands IGNORE, INCLUDE and REJECT, selection criteria
specified by the SET command will be considered for the next PLOT and
FIT commands. However, contrary to commands IGNORE, INCLUDE and REJECT,
the criteria will not be reset by any READ or FILE command.

7.11 SHOW

[POINT\]SHOW Item

 shows the specified items :
 RMS The maximum standard deviation of original measurements
 IGNORED Data points ignored based on Scans or Source name
 ELEVATION The elevation range
 REJECTED The rejected data scans, based on previous fit model

7.12 SOLVE

    [POINT\]SOLVE

     Compute fit results, considering only the valid data points implied
by commands IGNORE, REJECT, SET RMS or SET ELEVATION.

Index

FILE, 11

IGNORE, 11 INCLUDE, 11

LIST, 11

PARAMETER, 11 PLOT, 12 PRINT, 13

READ, 13 REJECT, 13

SET, 13 SHOW, 14 SOLVE, 14